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Read this operators guide carefully, before using the machine. Ensure that you know how the machine works, and how it should be operated. Maintain the machine in accordance with the instructions, and make certain that the machine functions correctly. Keep this operator’s guide and other enclosed documentation with the machine.
TECHNICAL SPECIFICATIONS                                        

	Model
	DB1900


	Rated Voltage
	220-240V ~ 50/60Hz

	Power
	1900W

	No load speed 
	2150/min

	impact frequency 
	1300/min

	Impact energy 
	45J

	Drill bits 
	SDS Hex 

	Net weight
	14kg 


Over view 
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1. switch trigger                         2. locking on button 

3.stop lever                             4.auxiliary handle 

5. oil gauge                             6.carbon brush holder cover
General Safety Instructions for Electric Tools

This device is exclusively for private use! It is not fit for commercial use!

WARNING! Read all instructions. Failure to follow all instructions listed below may result in electric shock, fire and/or serious injury:

SAVE THESE INSTRUCTIONS

1)Work area

• Keep work area clean and well lit. Cluttered and dark areas invite accidents

• Do not operate machines in explosive atmospheres, such as in the presence of flammable liquids, gases or dust. Machines create sparks which may ignite the dust or fumes.

• Keep children and bystanders away while operating a machine. Distractions can cause you to lose control.
2)Electrical safety

• Machine plugs must match the outlet. Never modify the plug in any way. Do not use any adapter plugs with earthed (grounded) machines. Unmodified plugs and matching outlets will reduce risk of electric shock.

• Avoid body contact with earthed or grounded surfaces such as pipes, radiators, ranges and refrigerators. There is an increased risk of electric shock if your body is earthed or grounded.

• Do not expose machines to rain or wet conditions. Water entering a machine will increase the risk of electric shock.

• Do not abuse the cord. Never use the cord for carrying, pulling or unplugging the machine. Keep cord away from heat, oil, sharp edges or moving parts. Damaged or entangled cords increase the risk of electric shock.

• When operating a machine outdoors, use an extension cord suitable for outdoor use. Use of a cord suitable for outdoor use reduces the risk of electric shock.

3)Personal safety

• Stay alert, Watch what you are doing and use common sense when operating a machine. Do not use a machine while you are tired or under the influence of drugs, alcohol or medication. A moment of inattention while operating machines may result in serious personal injury.
• Use safety equipment. Always wear eye protection. Safety equipment such as dust mark, non-skid  safety shoes, hard hat, or hearing protection used for appropriate conditions will reduce personal injuries.

•Avoid accidental starting. Ensure the switch is in the off position before plugging in. Carrying machines with your finger on the switch or plugging in machines that have the switch on invites accidents.

•Remove any adjusting key or wrench before turning the machine on. A wrench or a key left attached to a rotating part of the machine may result in personal injury.

•Do not overreach. Keep proper footing and balance at all times. This enables better control of the machine in unexpected situations.

• Dress properly. Do not wear loose clothing or jewellery. Keep your hair, clothing and gloves away from moving parts. Loose clothes, jewellery or long hair can be caught in moving parts.

• If devices are provided for the connection of dust extraction and collection facilities, ensure these are connected and properly used. Use of these devices can reduce dust related hazards.

4)Machine use and care

• Do not force the machine. Use the correct machine for your application. The correct machine will do the job better and safer at the rate for which it was designed.

•Do not use the machine if the switch does not turn it on and off. Any machine that can not be controlled with the switch is dangerous and must be repaired.

•Disconnect the plug from the power source before making any adjustments, changing accessories, or storing machines. Such preventive safety measures reduce the risk of starting the machine accidentally.

• Store idle machines out of the reach children and do not allow persons unfamiliar with the machine or these instructions to operate the machine. Machines are dangerous in the hands of untrained users.

• Maintain machines. Check for misalignment or binding of moving parts, breakage of parts and any other condition that may affect the machines operation. If damaged, have the machine repaired before use. Many accidents are caused by poorly maintained machines.

•Keep cutting tools sharp and clean. Properly maintained cutting tools with sharp cutting edges are less likely to bind and are easier to control.

• Use the machine, accessories and tool bits etc., in accordance with these instructions and in the manner intended for the particular type of machine, taking into account the working conditions and the work to be performed. Use of the machine for operations different from intended could result in a hazardous situation.

5) Service

• Have your machine serviced by a qualified repair person using only identical replacement parts. This will ensure that the safety of the machine is maintained.
SPECIFIC SAFETY RULES FOR DEMOLITION BREAKER:

1. Wear ear protectors. Exposure to noise can cause hearing loss.
2. Use auxiliary handles supplied with the tool. Loss of control can cause personal injury. 
3. Hold power tools by insulated gripping surfaces when performing an operation where the cutting tool may contact hidden wiring or its own cord. Contact with a "live" wire will make exposed metal parts of the tool "live" and shock the operator. 
4. Wear a hard hat (safety helmet), safety glasses and/or face shield. Ordinary eye or sun glasses are NOT safety glasses. It is also highly recommended that you wear a dust mask and thickly padded gloves. 
5. Be sure the bit is secured in place before operation. 
6. Under normal operation, the tool is designed to produce vibration. The screws can come loose easily, causing a breakdown or accident. Check tightness of screws carefully before operation. 
7. In cold weather or when the tool has not been used for a long time, let the tool warm up for a while by operating it under no load. This will loosen up the lubrication. Without proper warm-up, hammering operation is difficult. 
8.  Always be sure you have a firm footing. Be sure no one is below when using the tool in high locations. 
9. Hold the tool firmly with both hands. 
10. Keep hands away from moving parts. 
11.  Do not leave the tool running. Operate the tool only when hand-held. 
12. Do not point the tool at any one in the area when operating. The bit could fly out and injure someone seriously. 
13.  Do not touch the bit or parts close to the bit immediately after operation; they may be extremely hot and could burn your skin. Some material contains chemicals which may be toxic. Take caution to prevent dust inhalation and skin contact. Follow material supplier safety data.
OPERATION INSTRUCTIONS                                         
A. mounting chisel 

Rotate the stop lever (1) 180°clockwise direction while pulling it toward you. Then insert the chisel into the hexagonal hole on the frontcover. Clamp the tool by turning the stop lever 180°in the opposite direction. 
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B. power ON/off

Press the switch trigger to power on. If you need use continuous, press the locking on button to lock the switch after prssed the switch trigger. Press and release the switch trigger to power off.

C.oil feeding 

Since an oil chamber, it needn't be feed oil before be used for approximately 60 hours.Feed oil into the oil tank as described below:

1.just before no oil is visible in the oil gauge window (1)when the device is held upright.

2.before feeding oil, use the proveded allen key to remove the oil gauge(1).

3.check the oil level, confirm that oil is filled.

4.after feeding oil, put oil gauge (1)and screw back four screws.
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MAINTENANCE
•Always be sure that the tool is switched off and unplugged before attempting to perform inspection or maintenance.
To maintain product SAFETY and RELIABILITY, repairs, carbon brush inspection and replacement, any other maintenance or adjustment should be performed by Authorized or Factory Service Centers, always using our replacement parts.
ENVIRONMENTAL PROTECTION

[image: image11.emf]Electrical products should not be disposed of with household waste.

Please recycle where facilities exist. Check with your local authority or retailer for recycling advice.
DB1900 exploded view                           
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DB1900  part list 
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